|  |
| --- |
| Declaration of Performance.TROPIC MUURSERRE |
| CE conformity marking | C:\Users\gsd8301\Dropbox\FusionPoint\EN 1090\CE logo.jpg |
| Identification number of the notified body: | 1148 |
| Name and registeredaddress of the manufacturer (4): | Euroserre NVGeleenlaan 1 – 3600 Genk |
| The year in which themarking was affixed: | 2023 |
| Certificate number: | 1148-CPR-20231003-989 |
| **EN 1090-1:2009 + A1:2011** | EN 1090-3 | EXC1 |
| **Design** | MPCS |
| Project: identification code of the product-type / (1) | Tropic Muurserre |
| Serial number (2) | - |
| Method of declaration of properties: | Method 1 |
| 1. Unique identification code of the product-type: cfr. supra
2. Type, batch or serial number, or other means of identifying the construction product, as prescribed in Article 11(4): cfr. supra
3. Intended use or uses of the construction product, in accordance with the applicable harmonised technical specification, as foreseen by the manufacturer: Prefabricated construction kits for hobby greenhouses for use according to the construction products regulation EU 305/2011.
4. Name, registered trade name or registered trade mark and contact address of the manufacturer as required pursuant to Article 11(5): cfr. supra (3)
5. Where applicable, name and contact address of the authorised representative whose mandate covers the tasks specified in Article 12(2): Not applicable.
6. System or systems of assessment and verification of constancy of performance of the construction product as set out in Annex V: System 2+.
7. In case of the declaration of performance concerning a construction product covered by a harmonised standard: OCAB-OCBS, NoBo 1148 performed the initial inspection of the manufacturing plant and of factory production control according to EN 1090-1 under System 2+ and issued the certificate of conformity of the factory production control with reference 1148-CPR-2023-989.
8. If the declaration of performance relates to a construction product for which a European Technical Assessment has been issued: not applicable
9. Declared performances:
 |
| **Performance characteristic** | **Declaration** | **Harmonised technical specifications****EN 1090-1:2009 + A1:2011** |
| Tolerances on dimensions andshape | Functional tolerances: EN 1090-3 Annex GFunctional tolerances: EN 1090-3 Annex F | 4.2 | 5.3 |
| Base materials | EN 15088 EN AW 6060 | 4.3 | 5.4 |
| Fracture toughness, | NPD | 4.4 ; 4.8 | 5.5 ; 5.10 |
| Load bearing capacity | NPD | 4.5.2 | 5.6 |
| Fatigue strength | NPD | 4.5.3 | 5.6 |
| Resistance to fire | NPD | 4.5.4 | 5.7 |
| Reaction to fire | EN13501-1 Class A1 | 4.6 | 5.8 |
| Release of cadmium | NPD | 4.7 | 5.9 |
| Emission of radioactivity | NPD | 4.7 | 5.9 |
| Durability |  | 4.9 | 5.11 |
| If a Specific Technical Documentation has been used in accordance with Article 37 or 38, the requirements with which the product complies: not applicable. |
| 1. The performance of the product described in points 1 and 2 is in conformity with the performance indicated in point 9. This declaration of performance is issued in accordance with CPR (EU) 305/2011 under the sole responsibility of the manufacturer referred to in point 4.
 |
| Afbeelding met vlucht, schets, buitenshuis  Automatisch gegenereerde beschrijvingSigned for and on behalf of the manufacturer: Genk at 05.10.2023Dhr. Lemmens, C.E.O. , Euro-serre NV  |