|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Declaration of Performance.TROPIC MUURSERRE | | | | |
| CE conformity marking | | C:\Users\gsd8301\Dropbox\FusionPoint\EN 1090\CE logo.jpg | | |
| Identification number of the notified body: | | 1148 | | |
| Name and registered  address of the manufacturer (4): | | Euroserre NV  Geleenlaan 1 – 3600 Genk | | |
| The year in which the  marking was affixed: | | 2023 | | |
| Certificate number: | | 1148-CPR-20231003-989 | | |
| **EN 1090-1:2009 + A1:2011** | | EN 1090-3 | EXC1 | | |
| **Design** | | MPCS | | |
| Project: identification code of the product-type / (1) | | Tropic Muurserre | | |
| Serial number (2) | | - | | |
| Method of declaration of properties: | | Method 1 | | |
| 1. Unique identification code of the product-type: cfr. supra 2. Type, batch or serial number, or other means of identifying the construction product, as prescribed in Article 11(4): cfr. supra 3. Intended use or uses of the construction product, in accordance with the applicable harmonised technical specification, as foreseen by the manufacturer: Prefabricated construction kits for hobby greenhouses for use according to the construction products regulation EU 305/2011. 4. Name, registered trade name or registered trade mark and contact address of the manufacturer as required pursuant to Article 11(5): cfr. supra (3) 5. Where applicable, name and contact address of the authorised representative whose mandate covers the tasks specified in Article 12(2): Not applicable. 6. System or systems of assessment and verification of constancy of performance of the construction product as set out in Annex V: System 2+. 7. In case of the declaration of performance concerning a construction product covered by a harmonised standard: OCAB-OCBS, NoBo 1148 performed the initial inspection of the manufacturing plant and of factory production control according to EN 1090-1 under System 2+ and issued the certificate of conformity of the factory production control with reference 1148-CPR-2023-989. 8. If the declaration of performance relates to a construction product for which a European Technical Assessment has been issued: not applicable 9. Declared performances: | | | | |
| **Performance characteristic** | **Declaration** | | **Harmonised technical specifications**  **EN 1090-1:2009 + A1:2011** | |
| Tolerances on dimensions and  shape | Functional tolerances: EN 1090-3 Annex G  Functional tolerances: EN 1090-3 Annex F | | 4.2 | 5.3 |
| Base materials | EN 15088 EN AW 6060 | | 4.3 | 5.4 |
| Fracture toughness, | NPD | | 4.4 ; 4.8 | 5.5 ; 5.10 |
| Load bearing capacity | NPD | | 4.5.2 | 5.6 |
| Fatigue strength | NPD | | 4.5.3 | 5.6 |
| Resistance to fire | NPD | | 4.5.4 | 5.7 |
| Reaction to fire | EN13501-1 Class A1 | | 4.6 | 5.8 |
| Release of cadmium | NPD | | 4.7 | 5.9 |
| Emission of radioactivity | NPD | | 4.7 | 5.9 |
| Durability |  | | 4.9 | 5.11 |
| If a Specific Technical Documentation has been used in accordance with Article 37 or 38, the requirements with which the product complies: not applicable. | | | | |
| 1. The performance of the product described in points 1 and 2 is in conformity with the performance indicated in point 9. This declaration of performance is issued in accordance with CPR (EU) 305/2011 under the sole responsibility of the manufacturer referred to in point 4. | | | | |
| Afbeelding met vlucht, schets, buitenshuis  Automatisch gegenereerde beschrijvingSigned for and on behalf of the manufacturer: Genk at 05.10.2023  Dhr. Lemmens, C.E.O. , Euro-serre NV | | | | |